Word Algorithm for driviing

We get the starting position of the vehicle;

We check if the robot is driveable on Water,

if Yes, we call the A function and declare water as a safe path, else

we declare water as obstacle or undriveable path

we call the Astar function,

The robot follows the shortest path to the goal position(Where the object to be rescued is located),D